Tingkatkan standar kualitas produk Anda dengan UV Test Chamber multifungsi kami, sebuah solusi inovatif yang dirancang untuk mensimulasikan panas matahari dan radiasi ultraviolet secara akurat. Alat ini secara spesifik digunakan untuk mengobservasi tingkat ketahanan material terhadap efek menguning (yellowing) akibat paparan sinar UV dan suhu dalam jangka waktu tertentu. Dengan kemampuan untuk menilai perubahan warna secara presisi, mesin ini menjadi instrumen vital untuk menjamin estetika dan daya tahan produk, khususnya untuk material berwarna terang atau putih.
Keunggulan utama alat ini terletak pada fleksibilitasnya yang luar biasa. Tidak hanya berfungsi sebagai chamber pengujian UV, mesin canggih ini juga dapat dioperasikan sebagai aging tester (alat uji penuaan) dan oven laboratorium konvensional dengan rentang temperatur yang luas, mencapai hingga 200°C. Fungsi tiga-dalam-satu ini menjadikannya investasi yang sangat efisien, menghemat ruang dan biaya pengadaan peralatan di laboratorium atau fasilitas quality control Anda, sambil menyediakan kapabilitas pengujian yang beragam.
Dibangun untuk hasil yang cepat dan akurat, chamber ini dilengkapi dengan lampu UV berdaya 300W yang kuat untuk mempercepat proses pengujian secara signifikan. Fitur rak uji berputar yang kecepatannya dapat disesuaikan (1-10 rpm) memastikan setiap sisi sampel menerima paparan panas dan sinar UV yang seragam dan merata. Kontrol temperatur digital PID yang sangat akurat menjamin stabilitas suhu, sementara kepatuhannya terhadap standar internasional seperti ASTM D1148 dan ISO8580 memberikan validitas yang tak terbantahkan pada setiap hasil pengujian Anda.
Mengadopsi mesin uji ini ke dalam proses R&D dan quality assurance Anda adalah langkah strategis untuk menjaga nilai merek dan kepuasan pelanggan. Dengan kemampuan untuk secara proaktif menguji dan mencegah masalah menguning, Anda dapat memastikan produk akhir mempertahankan warna aslinya lebih lama, bahkan setelah terpapar kondisi lingkungan yang ekstrem. Jadikan alat uji multifungsi yang andal ini sebagai garda terdepan Anda dalam menciptakan produk berkualitas superior.
Elevate your product quality standards with our multi-function UV Test Chamber, an innovative solution designed to accurately simulate solar heat and ultraviolet radiation. This machine is specifically used to observe the anti-yellowing degree of materials after exposure to UV light and temperature over a period. With the ability to precisely judge color changes, this instrument is vital for guaranteeing the aesthetics and durability of products, especially for light-colored or white materials.
The primary advantage of this device lies in its exceptional flexibility. It does not only function as a UV testing chamber; this advanced machine can also be operated as an aging tester and a conventional laboratory oven with a wide temperature range reaching up to 200°C. This three-in-one functionality makes it a highly efficient investment, saving valuable space and equipment costs in your laboratory or quality control facility while providing diverse testing capabilities.
Engineered for rapid and accurate results, this chamber is equipped with a powerful 300W UV lamp to significantly accelerate the testing process. A rotating test rack with adjustable speed (1-10 rpm) ensures that every side of the sample receives uniform and even exposure to heat and UV radiation. The highly accurate digital PID temperature controller guarantees temperature stability, while its compliance with international standards like ASTM D1148 and ISO8580 provides undeniable validity to every test result.
Adopting this test machine into your R&D and quality assurance process is a strategic move to protect your brand value and customer satisfaction. With the ability to proactively test and prevent yellowing issues, you can ensure your final products retain their original color for longer, even after being exposed to extreme environmental conditions. Make this reliable, multi-function test instrument your frontline defense in creating products of superior quality.

