Kami menyediakan rangkaian lengkap alat uji kekerasan digital, mencakup metode Rockwell dan Vickers, untuk memenuhi semua kebutuhan analisis material dan quality control Anda. Kekerasan adalah parameter krusial yang menentukan kualitas dan fungsi mekanis sebuah komponen logam. Dengan instrumen kami, Anda dapat secara akurat menilai berbagai sifat turunan material seperti kekuatan, ketahanan aus, dan ketahanan lelah. Baik untuk inspeksi cepat di lini produksi maupun analisis mikro yang mendalam di laboratorium R&D, kami memiliki solusi pengujian yang tepat untuk memastikan integritas produk Anda.
Digital Rockwell Hardness Tester kami adalah pilihan ideal untuk pengujian yang cepat dan efisien. Alat ini bekerja dengan mengukur kedalaman penetrasi indenter di bawah beban yang spesifik, memberikan hasil pembacaan langsung pada layar digital yang jernih, seperti dalam skala HRC (Hardness Rockwell C) untuk baja yang dikeraskan. Sesuai fungsinya, alat ini sangat efektif untuk quality control pada komponen hasil proses perlakuan panas (heat treatment) dan material logam secara umum, memberikan data yang cepat dan dapat diandalkan untuk memastikan konsistensi produksi.
Untuk kebutuhan pengujian yang lebih presisi dan serbaguna, Digital Vickers Hardness Tester kami menawarkan teknologi canggih yang mengintegrasikan sistem optik, mekanik, dan elektronik. Metode Vickers menggunakan indenter intan berbentuk piramida untuk membuat jejak mikro pada permukaan sampel, yang kemudian diukur secara presisi melalui sistem optik. Spesifikasi ini membuatnya unggul untuk menguji material yang sangat tipis, spesimen kecil, lapisan permukaan (coating), dan untuk analisis kekerasan pada area mikrostruktur material, memberikan data yang sangat detail dan akurat.
Dengan memiliki akses ke kedua metode pengujian ini, Anda mendapatkan kapabilitas quality assurance yang komprehensif. Gunakan tester Rockwell untuk kecepatan dan kemudahan pada pengujian makro, dan andalkan tester Vickers untuk presisi dan detail pada pengujian mikro. Kedua instrumen digital ini dirancang untuk keandalan, kemudahan operasional, dan hasil yang akurat, menjadikannya investasi fundamental untuk memvalidasi kualitas material dan menjamin performa superior dari setiap produk yang Anda hasilkan.
We provide a complete range of digital hardness testers, featuring both the Rockwell and Vickers methods, to meet all your material analysis and quality control needs. Hardness is a crucial parameter that determines the quality and mechanical function of a metallic component. With our instruments, you can accurately infer various derivative material properties such as strength, wear resistance, and fatigue life. Whether for rapid inspection on the production line or for in-depth micro-analysis in the R&D lab, we have the right testing solution to ensure your product's integrity.
Our Digital Rockwell Hardness Tester is the ideal choice for fast and efficient testing. This instrument operates by measuring the penetration depth of an indenter under a specific load, providing a direct readout on a clear digital display, such as on the HRC (Hardness Rockwell C) scale for hardened steels. As per its function, this device is highly effective for quality control on parts that have undergone heat treatment and for general metallic materials, delivering quick and reliable data to ensure production consistency.
For more precise and versatile testing needs, our Digital Vickers Hardness Tester offers advanced technology that integrates optical, mechanical, and electronic systems. The Vickers method utilizes a pyramid-shaped diamond indenter to create a micro-indentation on the sample's surface, which is then precisely measured via an optical system. This specification makes it superior for testing very thin materials, small specimens, surface layers (coatings), and for analyzing the hardness of specific microstructural areas, providing highly detailed and accurate data.
By having access to both testing methods, you gain a comprehensive quality assurance capability. Use the Rockwell tester for speed and simplicity in macro testing, and rely on the Vickers tester for precision and detail in micro testing. Both digital instruments are designed for reliability, operational ease, and accurate results, making them a fundamental investment to validate material quality and guarantee the superior performance of every product you manufacture.

