Kami menyediakan rangkaian solusi uji kekerasan makro yang komprehensif, menampilkan dua metode pengujian paling fundamental di industri: Brinell dan Rockwell. Kedua instrumen ini adalah pilar utama dalam laboratorium quality control dan manufaktur, dirancang untuk memastikan setiap material, mulai dari besi cor mentah hingga komponen baja yang telah melalui perlakuan panas, memenuhi spesifikasi kekerasan yang tepat. Dengan menyediakan kedua metode ini, kami menawarkan kapabilitas pengujian yang lengkap untuk menjaga integritas dan kualitas produk Anda.
Electronic Brinell Hardness Tester kami adalah pilihan superior untuk mengukur material dengan struktur butiran yang kasar atau tidak homogen. Sesuai fungsinya, alat ini sangat ideal untuk pengujian pada besi cor (cast iron), produk baja, logam non-ferrous, dan paduan lunak (soft alloys). Metode Brinell bekerja dengan menekan bola indenter (carbide ball) ke permukaan sampel dan mengukur diameter jejak yang dihasilkan, memberikan nilai kekerasan rata-rata yang representatif di area yang luas. Selain itu, versatilitasnya memungkinkan pengujian pada beberapa material non-logam keras seperti plastik dan bakelite.
Di sisi lain, Rockwell Hardness Tester adalah standar industri untuk pengujian yang cepat, sederhana, dan sangat dapat diulang, terutama untuk verifikasi proses perlakuan panas. Alat ini sangat luas digunakan untuk memeriksa kekerasan material setelah proses quenching (pendinginan cepat), hardening (pengerasan), dan tempering. Metode Rockwell secara langsung mengukur kedalaman penetrasi indenter, sehingga hasilnya dapat diperoleh dengan sangat cepat, menjadikannya pilihan sempurna untuk kontrol kualitas di lini produksi yang sibuk pada material logam ferrous maupun non-ferrous.
Dengan menawarkan kedua alat uji kekerasan Brinell dan Rockwell, kami memberikan solusi total untuk laboratorium jaminan kualitas Anda. Gunakan metode Brinell untuk pengujian yang representatif pada bahan baku dan material berstruktur kasar, dan andalkan metode Rockwell untuk pemeriksaan yang cepat dan akurat pada komponen jadi dan hasil heat treatment. Dapatkan instrumen yang tepat untuk setiap aplikasi dan pastikan setiap material yang Anda proses memenuhi standar industri tertinggi dari awal hingga akhir.
We provide a comprehensive suite of macro hardness testing solutions, featuring two of the most fundamental testing methods in the industry: Brinell and Rockwell. These two instruments are the mainstays of any quality control and manufacturing lab, designed to ensure every material, from raw cast iron to finished heat-treated steel components, meets its precise hardness specification. By offering both methods, we deliver a complete testing capability to safeguard your product's integrity and quality.
Our Electronic Brinell Hardness Tester is the superior choice for measuring materials with coarse or inhomogeneous grain structures. As per its function, it is ideally suited for testing on cast iron, steel products, nonferrous metals, and soft alloys. The Brinell method works by pressing a carbide ball indenter into the sample's surface and measuring the resulting indentation's diameter, providing a representative average hardness value over a large area. Furthermore, its versatility extends to testing some hard non-metallic materials such as plastics and bakelite.
On the other hand, the Rockwell Hardness Tester is the industry standard for fast, simple, and highly repeatable testing, especially for verifying heat treatment processes. It is widely used to check the hardness of materials after quenching, hardening, and tempering. The Rockwell method directly measures the depth of indenter penetration, allowing for very rapid results. This makes it the perfect choice for high-volume quality control on the production line for both ferrous and non-ferrous metallic materials.
By offering both Brinell and Rockwell hardness testers, we provide a total solution for your quality assurance laboratory. Utilize the Brinell method for representative testing on raw and coarse-structured materials, and rely on the Rockwell method for fast, accurate checks on finished parts and heat-treated components. Get the right instrument for every application and ensure every material you process meets the highest industry standards from start to finish.

