Tentukan sifat alir (flow properties) dari produk pelumas dan bahan bakar Anda pada suhu rendah dengan Low Temperature Kinematic Viscometer kami. Instrumen semi-otomatis yang terspesialisasi ini dirancang untuk secara akurat mengukur viskositas kinematik dari cairan petroleum, baik yang transparan maupun buram. Pengujian ini sangat krusial untuk memprediksi performa produk di iklim dingin dan merupakan parameter kunci dalam spesifikasi kualitas. Seluruh desain dan operasional alat ini dibuat sesuai dengan metode uji standar internasional ASTM D445.
Inti dari performa alat ini adalah sistem kontrol temperatur presisi tingginya. Dilengkapi dengan teknologi pendingin kompresor yang kuat dan efisien, instrumen ini mampu mencapai dan menjaga suhu pengujian dalam rentang yang sangat luas, dari -60°C hingga +60°C. Pengontrol suhu digital yang canggih, dikombinasikan dengan sensor Pt100 yang sensitif, memastikan temperatur di dalam bak (bath) terjaga dengan akurasi luar biasa, yaitu ±0.1°C, menciptakan kondisi yang stabil dan ideal untuk pengukuran viskositas yang andal.
Dirancang untuk efisiensi dan kemudahan penggunaan, apparatus ini memiliki bak pendingin jenis Dewar dari kaca yang transparan dengan sistem pencahayaan internal, memungkinkan observasi yang jelas terhadap tabung viskometer kapiler selama pengujian. Penutup bak dengan beberapa lubang (multi-hole) dan klip viskometer model baru memungkinkan operator untuk menyiapkan dan menguji beberapa sampel secara paralel, sehingga secara signifikan meningkatkan produktivitas laboratorium. Motor pengaduk yang kuat (1200r/min) menjamin suhu di dalam bak berkapasitas 8L ini terdistribusi secara merata dan konstan.
Bagi laboratorium yang menganalisis sifat alir dingin (cold flow properties) pada oli mesin, oli hidrolik, bahan bakar jet, dan pelumas lainnya, viskometer ini adalah solusi yang andal dan efektif. Sifatnya yang semi-otomatis mengombinasikan presisi dari kontrol suhu digital dengan kesederhanaan pengukuran waktu manual, menawarkan sebuah paket yang tangguh dan bernilai tinggi. Pastikan produk Anda memenuhi spesifikasi performa suhu rendah yang ketat dengan data viskositas kinematik yang akurat dari instrumen esensial ini.
Determine the flow properties of your lubricant and fuel products at low temperatures with our Low Temperature Kinematic Viscometer. This specialized, semi-automatic instrument is designed to accurately measure the kinematic viscosity of liquid petroleum products, both transparent and opaque. This test is crucial for predicting product performance in cold climates and is a key quality specification parameter. The entire design and operation of this apparatus conform to the ASTM D445 international standard test method.
At the core of this instrument's performance is its high-precision temperature control system. Equipped with a powerful and efficient refrigeration compressor technology, it is capable of achieving and maintaining test temperatures over a very wide range, from -60°C to +60°C. An advanced digital temperature controller, combined with a sensitive Pt100 sensor, ensures the bath temperature is maintained with exceptional accuracy of ±0.1°C, creating a stable and ideal condition for reliable viscosity measurements.
Designed for efficiency and ease of use, the apparatus features a transparent Dewar-type glass cold bath with an internal lighting system, allowing for clear observation of the capillary viscometer tubes during the test. The multi-hole bath cover and new, easy-to-use viscometer clips allow the operator to prepare and run several samples in parallel, thus significantly increasing laboratory productivity. A powerful motor stirrer (1200r/min) guarantees that the temperature within the 8L bath is evenly and constantly distributed.
For laboratories analyzing the cold flow properties of engine oils, hydraulic oils, jet fuels, and other lubricants, this viscometer is a reliable and effective solution. Its semi-automatic nature combines the precision of digital temperature control with the simplicity of manual timing, offering a robust and high-value package. Ensure your products meet stringent low-temperature performance specifications with accurate kinematic viscosity data from this essential instrument.

