Tingkatkan kapabilitas laboratorium analisis oli Anda dengan Automatic TAN/TBN Titrator kami, sebuah instrumen canggih yang dirancang untuk analisis produk perminyakan. Alat ini memiliki fungsi ganda yang krusial: menentukan secara akurat Total Acid Number (TAN) atau Angka Asam Total, dan Total Base Number (TBN) atau Angka Basa Total, melalui metode titrasi potensiometrik. Pengujian ini sangat vital untuk memonitor degradasi oli, menilai sisa masa pakai pelumas (remaining useful life), dan memastikan oli layak pakai. Instrumen ini sepenuhnya sesuai dengan standar industri esensial, yaitu ASTM D664 (TAN) dan ASTM D2896 (TBN).
Presisi adalah fondasi dari setiap komponen dalam titrator ini. Sistem penyaluran volume dikendalikan oleh closed-loop control yang presisi, menggerakkan buret berakurasi tinggi dengan ketelitian hingga 0.005mm. Katup solenoida dengan desain zero-dead volume memastikan tidak ada reagen yang terbuang dan meningkatkan akurasi titik akhir titrasi. Dengan repetabilitas analisis sebesar 0.2% dan sensitivitas kontrol titrasi ±2mV, Anda dapat memiliki kepercayaan penuh pada setiap hasil yang dikeluarkan oleh mesin ini untuk keputusan pemeliharaan yang kritis.
Dirancang untuk kemudahan dan efisiensi di laboratorium modern, alat ini dioperasikan melalui layar sentuh LCD yang intuitif, menyederhanakan proses pengaturan pengujian, pemantauan kurva titrasi, dan peninjauan data. Inovasi juga terlihat pada sistem pengaduknya yang menggunakan perangkat pengaduk magnetik ultrathin, memastikan sampel terhomogenisasi dengan sempurna tanpa kontak mekanis. Dengan empat elektroda khusus yang disertakan, instrumen ini siap digunakan untuk melakukan pengujian TAN dan TBN secara langsung.
Bagi laboratorium yang menjalankan program pemeliharaan prediktif (predictive maintenance), quality control oli baru, atau riset dan pengembangan, titrator ini adalah sebuah investasi yang sangat berharga. Kemampuannya untuk menjalankan dua jenis pengujian oli paling kritis pada satu platform dapat menghemat ruang, waktu, dan biaya. Dapatkan data yang akurat dan andal untuk mencegah korosi, keausan berlebih, dan kerusakan mesin yang mahal dengan instrumen analisis oli yang canggih ini.
Enhance the capabilities of your oil analysis laboratory with our Automatic TAN/TBN Titrator, a sophisticated instrument designed for the analysis of petroleum products. This device serves a crucial dual function: to accurately determine both the Total Acid Number (TAN) and the Total Base Number (TBN) via potentiometric titration. These tests are vital for monitoring oil degradation, assessing the remaining useful life of lubricants, and ensuring oils are fit for service. The instrument is in full compliance with the essential industry standards, ASTM D664 (for TAN) and ASTM D2896 (for TBN).
Precision is the foundation of every component in this titrator. The volume dispensing system is governed by a precise closed-loop control, driving a high-accuracy burette with a resolution of up to 0.005mm. A zero-dead volume solenoid valve ensures no reagent is wasted and improves the accuracy of the titration endpoint. With a high analysis repeatability of 0.2% and a titration control sensitivity of ±2mV, you can have complete confidence in every result produced by this machine for your critical maintenance decisions.
Designed for ease of use and efficiency in the modern laboratory, this instrument is operated via an intuitive LCD touch screen, which simplifies test setup, titration curve monitoring, and data review. Innovation is also evident in its stirring system, which utilizes an ultrathin magnetic stirring device to ensure perfect sample homogenization without mechanical contact. With four specialized electrodes included, the instrument is ready to perform both TAN and TBN tests right out of the box.
For laboratories running predictive maintenance programs, new oil quality control, or research and development, this titrator is an invaluable investment. Its ability to perform two of the most critical in-service oil tests on a single platform saves space, time, and cost. Obtain the accurate and reliable data needed to prevent corrosion, excessive wear, and costly machinery damage with this advanced oil analysis instrument.

