Pastikan kualitas dan keamanan tertinggi bahan bakar penerbangan Anda dengan Automatic Water Reaction Tester kami. Instrumen canggih ini dirancang khusus untuk menguji keberadaan komponen yang dapat larut dalam air (water-miscible components) pada bahan bakar aviasi seperti avtur (turbine fuel) dan bensin avigasi. Alat ini secara akurat mengevaluasi efek dari komponen tersebut terhadap perubahan volume dan kondisi antarmuka bahan bakar-air, sebuah parameter krusial untuk mencegah masalah pada sistem bahan bakar pesawat. Seluruh proses pengujian berjalan secara otomatis dan sepenuhnya sesuai dengan metode standar ASTM D1094.
Kunci dari kinerja alat ini adalah sistem pengocokan vertikal (vertical reciprocating motion) berkecepatan tinggi yang presisi dan ditenagai oleh gas. Seluruh proses, mulai dari periode dan rute eksperimental hingga penghitungan jumlah putaran, dikendalikan secara akurat oleh sistem mikrokomputer. Fleksibilitasnya memungkinkan pengguna untuk mengatur berbagai parameter pengujian, termasuk amplitudo (120-250mm), kecepatan (2-4 kali/detik), dan waktu pengocokan, yang kemudian diikuti dengan periode diam (quiescent time) selama 5 menit yang diatur secara otomatis sebelum alarm berbunyi.
Dirancang untuk kemudahan penggunaan dan akurasi observasi, alat ini dilengkapi dengan sumber cahaya LED lembut yang memberikan penerangan optimal untuk mengamati hasil dengan nyaman di berbagai kondisi lingkungan. Manajemen data menjadi sangat efisien; hasil pengujian disimpan secara otomatis dan dapat diunggah ke komputer melalui terminal komunikasi RS232 untuk analisis lebih lanjut atau pengarsipan. Selain itu, mikro-printer termosensitif yang terintegrasi memungkinkan Anda untuk mencetak laporan hasil secara langsung di tempat.
Bagi kilang minyak, terminal distribusi bahan bakar, depot militer, dan laboratorium quality control aviasi, instrumen otomatis ini adalah sebuah investasi vital. Dengan mengotomatiskan metode uji ASTM D1094 yang krusial, alat ini meningkatkan repetabilitas hasil, mengurangi variabilitas antar operator, dan secara signifikan meningkatkan efisiensi laboratorium. Pastikan bahan bakar jet Anda bebas dari kontaminan larut air yang berbahaya dan jaga integritas serta keamanan sistem bahan bakar pesawat dengan alat uji yang andal ini.
Ensure the highest quality and safety of your aviation fuels with our Automatic Water Reaction Tester. This advanced instrument is specifically designed to test for the presence of water-miscible components in aviation fuels such as turbine fuel (jet fuel) and aviation gasoline. It accurately evaluates the effect of these components on volume change and on the fuel-water interface, a crucial parameter for preventing issues in aircraft fuel systems. The entire testing process is fully automated and in strict conformity with the ASTM D1094 standard test method.
The key to this instrument's performance is its precise, gas-driven, high-speed vertical reciprocating motion system. The entire process, from the experimental period and route to the calculation of round-trips, is accurately controlled by a microcomputer system. Its flexibility allows users to adjust various test parameters, including amplitude (120-250mm), speed (2-4 times/s), and shaking time, which is then automatically followed by a 5-minute quiescent time before an alarm sounds.
Designed for ease of use and observational accuracy, the apparatus is equipped with a soft LED light source that provides optimal illumination for comfortably observing the results in different environmental conditions. Data management is highly efficient; results are saved automatically and can be uploaded to a computer via the RS232 communication terminal for further analysis or archiving. Furthermore, an integrated thermosensitive micro-printer allows you to print reports directly on-site.
For refineries, fuel distribution terminals, military depots, and aviation quality control labs, this automatic instrument is a vital investment. By automating the crucial ASTM D1094 test method, this apparatus improves result repeatability, reduces inter-operator variability, and significantly increases laboratory efficiency. Ensure your jet fuel is free from harmful water-soluble contaminants and safeguard the integrity and safety of aircraft fuel systems with this reliable testing tool.

