Dirancang untuk memenuhi tuntutan pengujian material yang paling berat, Mesin Uji Universal tipe lantai ini adalah solusi andal untuk analisis properti mekanis statis. Dengan kapasitas gaya uji maksimum mencapai 100KN , instrumen ini mampu secara akurat melakukan pengujian kekuatan tarik, tekan, lentur, dan geser pada berbagai material, termasuk logam dan komposit. Ini adalah perangkat esensial untuk laboratorium kontrol kualitas industri, lembaga penelitian, dan institusi akademik yang memerlukan data uji yang valid dan konsisten.
Kekuatan dan presisi menjadi inti dari rekayasa mesin ini, yang ditenagai oleh motor servo AC performa tinggi dari Jepang serta sabuk sinkron yang menggerakkan dua buah 
ball screw presisi tinggi tanpa celah. Sistem penggerak canggih ini menjamin stabilitas luar biasa, efisiensi tinggi, tingkat kebisingan rendah, dan akurasi kecepatan yang memenuhi standar ±0.5%. Pengukuran gaya didukung oleh sensor beban 100KN dengan akurasi kelas 0.5 , memberikan hasil yang dapat diandalkan pada rentang pengukuran 0.4% hingga 100% dari skala penuh.
Kecerdasan operasional diwujudkan melalui sistem pengukuran dan kontrol digital 
closed loop sepenuhnya. Perangkat lunak yang terhubung ke PC melalui USB memungkinkan pengguna untuk melakukan berbagai mode pengujian seperti uji siklus , serta secara otomatis menghitung parameter pengujian krusial seperti Rm dan E. Fitur visualisasi data yang canggih, termasuk fungsi 
zoom dan multi kurva , analisis data , dan kemampuan untuk menyimpan serta memanggil kembali data uji, menjadikan analisis hasil lebih mendalam dan efisien.
Dengan kemampuan menyediakan data pengujian yang sesuai dengan berbagai standar kalibrasi internasional seperti ISO 7500-1, ASTM E4, GB, DIN, dan JIS, mesin ini memastikan produk Anda siap untuk pasar global. Ruang uji efektif yang luas dengan lebar 590mm dan stroke efektif 720mm memberikan fleksibilitas untuk mengakomodasi beragam ukuran dan bentuk sampel. Investasikan pada instrumen ini untuk mendapatkan kepastian data, kepatuhan standar, dan keunggulan kompetitif dalam kualitas material.
Engineered to meet the most demanding material testing requirements, this floor model Universal Testing Machine is the definitive solution for static mechanical property analysis. With a maximum test force capacity of 100KN , this instrument is capable of accurately performing tensile, compression, flexure, and shear tests on a wide variety of materials, including metals and composites. It is an essential device for industrial quality control laboratories, research institutions, and academic facilities that require valid and consistent test data.
Power and precision are at the core of this machine's engineering, driven by a high-performance Japanese AC servo motor and a synchronous belt that actuates two high-precision, gapless ball screws. This advanced drive system ensures exceptional stability, high efficiency, low noise levels, and a speed accuracy that meets the ±0.5% standard. Force measurement is supported by a 100KN load sensor with an accuracy of class 0.5 , delivering reliable results across a measurement range of 0.4% to 100% of full scale.
Operational intelligence is embodied by the fully digital closed-loop measuring and control system. The software, connected to a PC via USB , allows users to perform various test modes like cycle testing and to automatically calculate crucial test parameters such as Rm and E. Advanced data visualization features, including zoom and multi-curve functionality , data analysis , and the ability to store and recall test data, make result analysis more insightful and efficient.
With the capability to provide test data in accordance with various international calibration standards like ISO 7500-1, ASTM E4, GB, DIN, and JIS, this machine ensures your products are ready for the global market. A generous effective testing width of 590mm and an effective stroke of 720mm provide the flexibility to accommodate diverse sample sizes and shapes. Invest in this instrument for data certainty, standards compliance, and a competitive edge in material quality.

