Kami menyediakan rangkaian lengkap Mesin Uji Material (Material Testing Machine) dan Mesin Uji Universal (UTM) untuk memenuhi semua kebutuhan pengujian kekuatan mekanis material Anda. Portofolio kami yang luas mencakup sistem elektromekanis dan hidrolik untuk uji tarik, tekan, dan lentur yang sesuai dengan berbagai standar internasional. Berikut adalah rincian konfigurasi dan rentang spesifikasi yang tersedia dalam portofolio kami.
Portofolio kami menawarkan rentang kapasitas gaya dan konfigurasi mesin yang sangat luas untuk disesuaikan dengan setiap aplikasi. Kapasitas beban tersedia mulai dari 10KN hingga 3000KN (300 Ton), ideal untuk pengujian material ringan seperti plastik dan tekstil hingga pengujian heavy-duty pada baja dan beton. Konfigurasi mesin mencakup sistem elektromekanis kolom tunggal (single column) yang ringkas, kolom ganda (double column) yang serbaguna, serta sistem hidrolik heavy-duty untuk pengujian kekuatan ultra-tinggi. Pilihan ini memastikan Anda mendapatkan mesin yang tepat sesuai dengan jenis material dan kekuatan yang akan diuji.
Sistem kami dirancang untuk melakukan berbagai mode pengujian mekanis yang paling fundamental. Kemampuan utamanya meliputi uji tarik (tensile test), uji tekan (compression test), dan uji lentur (flexure/bending test). Tergantung pada kebutuhan laboratorium Anda, kami menawarkan beberapa opsi sistem kontrol dan tampilan. Ini berkisar dari unit dengan tampilan dial gauge untuk pembacaan dasar, tampilan digital (digital display) untuk akurasi yang lebih tinggi dan kemudahan pembacaan, hingga sistem dengan kontrol penuh melalui PC yang dilengkapi perangkat lunak canggih untuk akuisisi data, penggambaran kurva tegangan-regangan, analisis mendalam, dan pelaporan otomatis.
Aplikasi dari rangkaian mesin uji material kami hampir tidak terbatas, mencakup berbagai sektor industri dan penelitian. Mesin-mesin ini secara rutin digunakan untuk menguji beragam material seperti logam, baja (termasuk untaian baja/steel strand), beton, plastik, karet, komposit, tekstil, dan banyak lagi. Setiap mesin dalam portofolio kami dirancang untuk memberikan hasil yang akurat, andal, dan dapat diulang, menjadikannya aset vital untuk kontrol kualitas (QC), riset dan pengembangan (R&D), serta sertifikasi produk di lingkungan akademik maupun industri.
We provide a complete range of Material Testing Machines and Universal Testing Machines (UTM) to meet all your mechanical strength testing needs. Our extensive portfolio includes electromechanical and hydraulic systems for tensile, compression, and flexure tests that comply with various international standards. The following are the detailed configurations and specification ranges available in our portfolio.
Our portfolio offers an extremely wide range of force capacities and machine configurations to suit every application. Load capacities are available from 10KN up to 3000KN (300 Tons), ideal for testing lightweight materials like plastics and textiles, all the way to heavy-duty testing of steel and concrete. Machine configurations include compact single-column electromechanical systems, versatile double-column models, and heavy-duty hydraulic systems for ultra-high-strength testing. This selection ensures you get the right machine for the material type and strength you need to test.
Our systems are designed to perform the most fundamental mechanical testing modes. Core capabilities include tensile tests, compression tests, and flexure/bending tests. Depending on your laboratory's requirements, we offer several control and display system options. These range from units with a dial gauge display for basic readings, a digital display for higher accuracy and ease of reading, to systems with full PC control featuring advanced software for data acquisition, stress-strain curve plotting, in-depth analysis, and automated reporting.
The applications for our range of material testing machines are nearly limitless, covering a multitude of industrial and research sectors. These machines are routinely used to test a diverse array of materials such as metals, steel (including steel strand), concrete, plastics, rubber, composites, textiles, and many more. Every machine in our portfolio is designed to deliver accurate, reliable, and repeatable results, making them vital assets for quality control (QC), research and development (R&D), and product certification in both academic and industrial environments.

